//Copyright (C)2014-2024 Gowin Semiconductor Corporation.
//All rights reserved. 
//File Title: Physical Constraints file
//Tool Version: V1.9.9.03 (64-bit)
//Part Number: GW1N-LV9PG256C6/I5
//Device: GW1N-9
//Created Time: Wed 02 26 18:14:50 2025

IO_LOC "FpgaLed_o" L16;
IO_PORT "FpgaLed_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DataMax2870MixRf2_o" C1;
IO_PORT "DataMax2870MixRf2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "ClkMax2870MixRf2_o" C2;
IO_PORT "ClkMax2870MixRf2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "CsMax2870MixRf2_o" D2;
IO_PORT "CsMax2870MixRf2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DataRegRf2_o" F16;
IO_PORT "DataRegRf2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "ClkRegRf2_o" E16;
IO_PORT "ClkRegRf2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "CsRegRf2_o" F15;
IO_PORT "CsRegRf2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "FpgaMosiAtt_o" C7;
IO_PORT "FpgaMosiAtt_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "FpgaClkAtt_o" B7;
IO_PORT "FpgaClkAtt_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "FpgaCsAtt_o" C8;
IO_PORT "FpgaCsAtt_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "AmDac2_mosi_o" B3;
IO_PORT "AmDac2_mosi_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "AmDac2Clk_o" A3;
IO_PORT "AmDac2Clk_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "AmDac2Cs_o" B4;
IO_PORT "AmDac2Cs_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "MosiPot_o" B5;
IO_PORT "MosiPot_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "ClkPot_o" A5;
IO_PORT "ClkPot_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "CsPot_o" A4;
IO_PORT "CsPot_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "MosiAd9912Fpga_o" R3;
IO_PORT "MosiAd9912Fpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "ClkAd9912Fpga_o" T2;
IO_PORT "ClkAd9912Fpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "CsAd9912Fpga_o" R4;
IO_PORT "CsAd9912Fpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DataLmx94_o" G1;
IO_PORT "DataLmx94_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "ClkLmx94_o" G2;
IO_PORT "ClkLmx94_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "CsLmx94_o" F1;
IO_PORT "CsLmx94_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "HrCtrlFpga_o" J16;
IO_PORT "HrCtrlFpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "FpgaAmCtrl_o" A15;
IO_PORT "FpgaAmCtrl_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DdsSaw1Fpga_o" E1;
IO_PORT "DdsSaw1Fpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "GpioAdRfV2_o" C16;
IO_PORT "GpioAdRfV2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "GpioAdRfV1_o" D16;
IO_PORT "GpioAdRfV1_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "RefOffsetCtrlFpga_o" P1;
IO_PORT "RefOffsetCtrlFpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DdsSaw2Fpga_o" D1;
IO_PORT "DdsSaw2Fpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DdsX2Fpga_o" R1;
IO_PORT "DdsX2Fpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "PllLoopCtrl_o" L1;
IO_PORT "PllLoopCtrl_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "PllSync_o" K2;
IO_PORT "PllSync_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "PllSyncCtrl_o" K1;
IO_PORT "PllSyncCtrl_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "PllVtuneCtrl_o" L2;
IO_PORT "PllVtuneCtrl_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "AmAlc1Fix_o" A2;
IO_PORT "AmAlc1Fix_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "SwCap1_o" A12;
IO_PORT "SwCap1_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "SwCap2_o" A10;
IO_PORT "SwCap2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "FpgaAlcDetSet_o" A11;
IO_PORT "FpgaAlcDetSet_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "AmAlcSw_o" A9;
IO_PORT "AmAlcSw_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "LrCtrlFpga_o" J15;
IO_PORT "LrCtrlFpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DdsSyncFpga_o" R6;
IO_PORT "DdsSyncFpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DdsResetFpga_o" T5;
IO_PORT "DdsResetFpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "DdsSyncCtrlFpga_o" T6;
IO_PORT "DdsSyncCtrlFpga_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "CtrlAmSw3_o" K16;
IO_PORT "CtrlAmSw3_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "RfSw2_o" G16;
IO_PORT "RfSw2_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "RfSw1_o" H16;
IO_PORT "RfSw1_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_PORT "AnyFlag_o" IO_TYPE=LVCMOS33;
IO_LOC "RfLd_o" R9;
IO_PORT "RfLd_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "I2cScl_o" T8;
IO_PORT "I2cScl_o" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "I2cSda_io" T7;
IO_PORT "I2cSda_io" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "Mosi1_io" T12;
IO_PORT "Mosi1_io" IO_TYPE=LVCMOS33 PULL_MODE=UP DRIVE=8 BANK_VCCIO=3.3;
IO_LOC "MisoLdMax2870_i" B1;
IO_PORT "MisoLdMax2870_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "MisoDds_i" T3;
IO_PORT "MisoDds_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "MisoLdLmx_i" F2;
IO_PORT "MisoLdLmx_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Mosi3_i" T15;
IO_PORT "Mosi3_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Mosi2_i" T14;
IO_PORT "Mosi2_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Mosi0_i" R12;
IO_PORT "Mosi0_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Ss_i" R8;
IO_PORT "Ss_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Sck_i" T13;
IO_PORT "Sck_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Rst_i" T9;
IO_PORT "Rst_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
IO_LOC "Clk_i" H11;
IO_PORT "Clk_i" IO_TYPE=LVCMOS33 PULL_MODE=UP BANK_VCCIO=3.3;
