{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Модуль RF","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":16,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Модуль RF","index":0,"n_rows":208,"n_cols":41,"rows_kept":208,"cut":false,"hidden":false,"merged":[[55,28,55,29],[55,31,55,32],[55,34,55,35],[10,23,10,32],[11,23,11,32],[12,23,12,32],[13,23,13,32],[14,23,14,32],[13,33,13,38],[14,33,14,38],[15,33,15,38],[16,33,16,38],[12,33,12,38],[167,15,167,22],[171,13,174,13],[171,15,172,38],[174,15,174,22],[178,13,181,13],[157,15,158,38],[152,15,153,38],[147,15,148,38],[121,14,122,37],[113,14,114,37],[100,14,101,37],[106,30,107,37],[68,14,97,45],[9,15,9,18],[9,19,9,22],[10,15,10,18],[10,19,10,22],[9,23,9,32],[12,15,12,18],[12,19,12,22],[204,13,207,13],[204,15,205,38],[185,13,188,13],[185,15,186,38],[188,15,188,30],[192,15,193,38],[197,15,198,38],[192,13,200,13],[195,15,195,30],[178,15,179,38],[181,15,181,22],[142,15,143,38],[142,13,160,13],[145,15,145,30],[164,13,167,13],[164,15,165,38],[17,15,17,18],[1,7,1,11],[2,7,9,11],[136,15,137,38],[136,13,139,13],[1,15,4,38],[6,15,7,18],[6,19,7,22],[8,15,8,18],[8,19,8,22],[6,23,7,32],[6,33,7,38],[8,23,8,32],[8,33,8,38],[11,15,11,18],[11,19,11,22],[14,15,14,18],[14,19,14,22],[16,15,16,18],[16,19,16,22],[9,33,9,38],[10,33,10,38],[13,15,13,18],[13,19,13,22],[11,33,11,38],[17,19,17,22],[16,23,16,32],[17,23,17,32],[18,15,18,18],[128,14,129,37],[15,15,15,18],[15,19,15,22],[20,15,28,38],[15,23,15,32],[30,15,38,38],[18,33,18,38],[18,19,18,22],[18,23,18,32],[17,33,17,38],[45,15,46,38],[48,16,48,20],[48,21,48,37],[52,15,53,38],[55,17,55,19],[55,21,55,22],[55,23,55,26]]}
[]
[{"$nulls":7},"Требования к сигналу сброса (RF_RST)",{"$nulls":7},"Общая характеристика модуля: \nMSB, 24bits, CLK = 10МГц"]
[{"$nulls":7},"1. После подачи питания на ПЛИС длительность задержки перед формированием начального сигнала сброса  - не менее 200 мкс.\n\n2. Длительность сигнала сброса не менее 600 нс."]
[]
[]
[]
[{"$nulls":15},"Имя объекта (Device ID)",null,null,null,"ID",null,null,null,"Параметры передачи",{"$nulls":9},"Примечание"]
[]
[{"$nulls":15},"LMX2594",null,null,null,0,null,null,null,"Длина слова 24 бита."]
[{"$nulls":15},"DDS",null,null,null,1,null,null,null,"Длина слова 80 бита."]
[{"$nulls":15},"POT",null,null,null,2,null,null,null,"Длина слова 16 бита."]
[{"$nulls":15},"ARM DAC",null,null,null,3,null,null,null,"Длина слова 16 бита."]
[{"$nulls":15},"ATT DAC",null,null,null,4,null,null,null,"Длина слова 16 бита."]
[{"$nulls":15},"SHIFT REG",null,null,null,5,null,null,null,"Длина слова 8 бит."]
[{"$nulls":15},"MAX2870",null,null,null,6,null,null,null,"Длина слова 32 бита."]
[{"$nulls":15},"GPIO1",null,null,null,7,null,null,null,"Длина слова 24 бита.",{"$nulls":9},"Запись в ПЛИС в режиме 1Mosi или 4Mosi"]
[{"$nulls":15},"TEMP",null,null,null,8,null,null,null,"Длина слова 24 бита.",{"$nulls":9},"Чтение из ПЛИС в режиме 1Mosi"]
[{"$nulls":15},"GPIO2",null,null,null,9,null,null,null,"Длина слова 24 бита.",{"$nulls":9},"Чтение из ПЛИС в режиме 1Mosi"]
[{"$nulls":15},"SERVICEINFO",null,null,null,10,null,null,null,"Длина слова 24 бита.",{"$nulls":9},"Версия программы и платы.Чтение  из ПЛИС в режиме 1Mosi"]
[]
[{"$nulls":15},"Описание работы в режиме 1 MOSI\nЗаголовок всегда длиной 24 бита. Последующие слова Payload могут иметь произвольное количество бит."]
{"$rows_empty":9}
[{"$nulls":15},"Описание работы в режиме 4 MOSI"]
{"$rows_empty":14}
[{"$nulls":15},"Заголовок для режима 1Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"MODE = 0","Device ID",{"$nulls":4},"Word counter",{"$nulls":16},"T=0/1"]
[]
[]
[]
[{"$nulls":15},"Заголовок для режима 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"MODE = 1",0,"DDS",null,null,0,"GPIO",null,"LMX2594",null,null,null,0,"MAX2870",null,0,"ShReg",null,0,"POT",null,"DAC","ATT","T=0/1"]
{"$rows_empty":12}
[{"$nulls":14},"MODE — Режим передачи данных\n      1 -4 MOSI\n      0 — 1 MISO/MOSI \nLoadOrder - Порядок отправки данных :\n0 - DDS->GPIO->LMX->MAX->ShReg->Pot->Dac->Att;\n1  - Lmx->Gpio->Dds->Max->ShReg->->Pot->Dac->Att. \nLMX2594 Word Cnt []  - Поле для задания кол-ва пакетов, которое необходимо отгрузить в  LMX2594 (11 регистров по 24 бита).\n\nDDS Word Cnt[] - Поле для задания кол-ва пакетов, которое необходимо отгрузить в DDS (1 регистр по 48 бит ).\n    \nPOT CNT []  - Поле для задания кол-ва пакетов, которое необходимо отгрузить в потенциометр.\n   \nDAC CNT []  - Поле для задания кол-ва пакетов, которое необходимо отгрузить в ЦАП.   \n\nShReg CNT []  - Поле для задания кол-ва пакетов, которое необходимо отгрузить в сдвиговый регистр .\n\nATT CNT []  - Поле для задания кол-ва пакетов, которое необходимо отгрузить в аттенюатор .\n    \nI2C[] -\n\nMAX2870[] -  Поле для задания кол-ва пакетов, которое необходимо отгрузить в MAX2870 \n\n"]
{"$rows_empty":31}
[{"$nulls":14},"GPIO1"]
[]
[{"$nulls":14},23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":14},"HR_CTRL_FPGA","FPGA_AM_CTRL","DDS_SAW1_FPGA","GPIO_ADRF_V2","GPIO_ADRF_V1","REF_OFFSET_CTRL_FPGA","DDS_SAW2_FPGA","DDS_X2_FPGA","PLL_LOOP_CTRL","PLL_SYNC","PLL_SYNC_CTRL","PLL_VTUNE_CTRL","AM_ALC_1_FIX","SW_CAP1","SW_CAP2","FPGA_ALC_DET_SET","AM_ALC_SW","LR_CTRL_FPGA","DDS_SYNC_FPGA","DDS_RESET_FPGA","DDS_SYNC_CTRL_FPGA","CTRL_AM_SW3","RF_SW2","RF_SW1"]
[]
[]
[{"$nulls":30},"Shift Register"]
[]
[{"$nulls":30},7,6,5,4,3,2,1,0]
[{"$nulls":30},"SW3_RF","SW2_RF","SW1_RF","SW_MIXER_RF","SW_0_15_RF","SW4_RF","SW_RF","SW_X2_RF"]
[]
[]
[]
[{"$nulls":14},"GPIO2"]
[]
[{"$nulls":14},23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":36},"LD_MAX","LD_LMX"]
[]
[]
[]
[]
[{"$nulls":14},"TempReg"]
[]
[{"$nulls":14},23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":14},"X","X","X","X","X","X","X","X","TEMP[10]","TEMP[9]","TEMP[8]","TEMP[7]","TEMP[6]","TEMP[5]","TEMP[4]","TEMP[3]","TEMP[2]","TEMP[1]","TEMP[0]","X","X","X","X","X"]
[]
[]
[]
[{"$nulls":14},"ServiceInfo"]
[]
[{"$nulls":14},23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0,null,null,"B-версия платы"]
[{"$nulls":14},"B[11]","B[10]","B[9]","B[8]","B[7]","B[6]","B[5]","B[4]","B[3]","B[2]","B[1]","B[0]","F[11]","F[10]","F[9]","F[8]","F[7]","F[6]","F[5]","F[4]","F[3]","F[2]","F[1]","F[0]",null,null,"F-версия прошивки"]
[]
[]
[]
[]
[{"$nulls":13},"LMX2594\nDATA",null,"Данные для LMX2594. Режим 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"LMX[23]","LMX[22]","LMX[21]","LMX[20]","LMX[19]","LMX[18]","LMX[17]","LMX[16]","LMX[15]","LMX[14]","LMX[13]","LMX[12]","LMX[11]","LMX[10]","LMX[9]","LMX[8]","LMX[7]","LMX[6]","LMX[5]","LMX[4]","LMX[3]","LMX[2]","LMX[1]","LMX[0]"]
[]
[]
[{"$nulls":13},"DDS\nDATA",null,"Данные для DDS. Режим 4Mosi (1)"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"X",{"$nulls":15},"DDS[79]","DDS[78]","DDS[77]","DDS[76]","DDS[75]","DDS[74]","DDS[73]","DDS[72]"]
[]
[{"$nulls":15},"Данные для DDS. Режим 4Mosi (2)"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"DDS[71]","DDS[70]","DDS[69]","DDS[68]","DDS[67]","DDS[66]","DDS[65]","DDS[64]","DDS[63]","DDS[62]","DDS[61]","DDS[60]","DDS[59]","DDS[58]","DDS[57]","DDS[56]","DDS[55]","DDS[54]","DDS[53]","DDS[52]","DDS[51]","DDS[50]","DDS[49]","DDS[48]"]
[]
[{"$nulls":15},"Данные для DDS. Режим 4Mosi (3)"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"DDS[47]","DDS[46]","DDS[45]","DDS[44]","DDS[43]","DDS[42]","DDS[41]","DDS[40]","DDS[39]","DDS[38]","DDS[37]","DDS[36]","DDS[35]","DDS[34]","DDS[33]","DDS[32]","DDS[31]","DDS[30]","DDS[29]","DDS[28]","DDS[27]","DDS[26]","DDS[25]","DDS[24]"]
[]
[{"$nulls":15},"Данные для DDS. Режим 4Mosi (4)"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"DDS[23]","DDS[22]","DDS[21]","DDS[20]","DDS[19]","DDS[18]","DDS[17]","DDS[16]","DDS[15]","DDS[14]","DDS[13]","DDS[12]","DDS[11]","DDS[10]","DDS[9]","DDS[8]","DDS[7]","DDS[6]","DDS[5]","DDS[4]","DDS[3]","DDS[2]","DDS[1]","DDS[0]"]
[]
[]
[]
[{"$nulls":13},"POT\nDATA",null,"Данные для POT. Режим 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"X",{"$nulls":7},"POT[15]","POT[14]","POT[13]","POT[12]","POT[11]","POT[10]","POT[9]","POT[8]","POT[7]","POT[6]","POT[5]","POT[4]","POT[3]","POT[2]","POT[1]","POT[0]"]
[]
[]
[]
[{"$nulls":13},"ARM DAC\nDATA",null,"Данные для ARM DAC. Режим 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"X",{"$nulls":7},"DAC[15]","DAC[14]","DAC[13]","DAC[12]","DAC[11]","DAC[10]","DAC[9]","DAC[8]","DAC[7]","DAC[6]","DAC[5]","DAC[4]","DAC[3]","DAC[2]","DAC[1]","DAC[0]"]
[]
[]
[]
[{"$nulls":13},"ATT\nDATA",null,"Данные для ATT. Режим 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"X",{"$nulls":7},"ATT[15]","ATT[14]","ATT[13]","ATT[12]","ATT[11]","ATT[10]","ATT[9]","ATT[8]","ATT[7]","ATT[6]","ATT[5]","ATT[4]","ATT[3]","ATT[2]","ATT[1]","ATT[0]"]
[]
[]
[]
[{"$nulls":13},"ShReg\nDATA",null,"Данные для SHIFT REG. Режим 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"X",{"$nulls":15},"ShReg[7]","ShReg[6]","ShReg[5]","ShReg[4]","ShReg[3]","ShReg[2]","ShReg[1]","ShReg[0]"]
[]
[]
[]
[{"$nulls":13},"MAX2870\nDATA",null,"Данные для MAX2870. Режим 4Mosi (1)"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"X",{"$nulls":15},"MAX[31]","MAX[30]","MAX[29]","MAX[28]","MAX[27]","MAX[26]","MAX[25]","MAX[24]"]
[]
[{"$nulls":15},"Данные для MAX2870. Режим 4Mosi (2)"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"MAX[23]","MAX[22]","MAX[21]","MAX[20]","MAX[19]","MAX[18]","MAX[17]","MAX[16]","MAX[15]","MAX[14]","MAX[13]","MAX[12]","MAX[11]","MAX[10]","MAX[9]","MAX[8]","MAX[7]","MAX[6]","MAX[5]","MAX[4]","MAX[3]","MAX[2]","MAX[1]","MAX[0]"]
[]
[]
[]
[{"$nulls":13},"GPIO\nDATA",null,"Данные для GPIO. Режим 4Mosi"]
[]
[{"$nulls":14},"Биты",23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":15},"GPIO[23]","GPIO[22]","GPIO[21]","GPIO[20]","GPIO[19]","GPIO[18]","GPIO[17]","GPIO[16]","GPIO[15]","GPIO[14]","GPIO[13]","GPIO[12]","GPIO[11]","GPIO[10]","GPIO[9]","GPIO[8]","GPIO[7]","GPIO[6]","GPIO[5]","GPIO[4]","GPIO[3]","GPIO[2]","GPIO[1]","GPIO[0]"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}