{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":33,"n_cols":19,"rows_kept":33,"cut":false,"hidden":false,"merged":[[3,1,4,1],[3,4,12,4],[3,5,8,5],[3,11,9,11],[5,2,15,2],[13,4,15,4],[10,11,15,11],[24,9,24,12],[24,13,24,17],[24,2,24,5],[24,6,24,8],[1,12,2,12],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,2,8],[1,9,2,9],[1,10,2,10],[1,11,2,11],[13,12,15,12],[17,2,17,5],[17,6,17,8],[17,9,17,12],[17,13,17,17],[10,12,12,12],[9,5,15,5],[18,11,18,12],[19,11,19,12],[20,11,20,12],[21,11,21,12],[22,11,22,12],[18,13,18,14],[19,13,19,14],[20,13,20,14],[21,13,21,14],[22,13,22,14]]}
[]
[null,"Fвых1,","FLMX,","Fвых2,","d","SW_RF","SW1_RF","SW2_RF","SW3_RF","SW4_RF","SW_MIXER_RF","GPIO_SW2_FILT_RF\n(GPIO_SW_015_RF)","GPIO_SW_FILT_RF\n(GPIO_SW_X2_RF)","GPIO_ADRF_V1"]
[null,"МГц","МГц","МГц",{"$nulls":9},"GPIO_ADRF_V2"]
[null,"0,1-1000(1250*)**","2750…3600",null,1,"“1”","“1”","“0”","-","-","“0”","“1”","-","-"]
[null,null,"3600…3999,9",null,null,null,"“0”","-","-",null,"“0”",null,"-","-"]
[null,"1000(1250*)-1300","-",null,null,null,"“1”","“1”","“1”","-","“1”",null,"-","-"]
[null,"1300-2200",{"$nulls":4},"“1”","“1”","“0”","-","“1”",null,"-","-"]
[null,"2200-3600",{"$nulls":4},"“1”","“0”","-","-","“1”",null,"-","-"]
[null,"3600-5500",{"$nulls":4},"“0”","-","-","-","“1”",null,"-","-"]
[null,"5500-6000",null,null,null,"“0”","-","-","-","“1”","-",null,"-","-"]
[null,null,null,"6000-7500",null,null,"-","-","-","“1”","-","“0”","“1”","“1”; “1” "]
[null,null,null,"7500-9000",null,null,"-","-","-","“1”","-",null,null,"“1”; “1” "]
[null,null,null,"9000-15000",null,null,"-","-","-","“0”","-",null,null,"“1”; “1” "]
[null,null,null,"15000-18000",2,null,"-","-","-","“1”","-",null,"“0”","“1”; “1” (0, 1)"]
[null,null,null,"18000-22000",null,null,"-","-","-","“0”","-",null,null,"“0”; “1”"]
[null,null,null,"22000-27000",null,null,"-","-","-","“0”","-",null,null,"“1”; “0”"]
[]
[null,null,"Разъем \"X3\" TMSG ",null,null,null,"Разъем 3pin \"J13\" ALINX",null,null,"Разъем \"X2\" TMSG ",null,null,null,"Разъем \"X1\" TMSG",{"$nulls":4},"Разъем 2pin ALINX"]
[null,"Частотный диапазон:","RF_SW1_GPIO","RF_SW2_GPIO","GND (№3)","CTRL_AM_SW3","GND (№1)","LrGpio(W16)","HrGpio(W15)","FPGA_AM_CTRL","GND (№2):","ATT_DAC",null,"ARM_DAC",null,null,"GND (№4):",null,"Mod(J15)"]
[null,"0 - 6 ГГц",0,0,0,0,0,"?","?",0,0,"0 - 65 535",null,"0 - 65 535",null,null,0,null,1]
[null,"6 - 27 ГГц",0,0,0,1,0,1,0,1,0,"0 - 65 535",null,"0 - 65 535",null,null,0,null,1]
[null,"27 - 37 ГГц",0,1,0,1,0,0,1,1,0,"0 - 65 535",null,"0 - 65 535",null,null,0,null,1]
[null,"37 - 45 ГГц",1,0,0,1,0,0,1,1,0,"0 - 65 535",null,"0 - 65 535",null,null,0,null,1]
[]
[null,null,"Разъем \"X5\": ",null,null,null,"Разъем \"X10\":",null,null,"Разъем \"X8\": ",null,null,null,"Разъем \"X7\":",{"$nulls":4},"Разъем \"X9\":"]
[null,"Частотный диапазон:","HF (№1)","LF (№2)","GND (№3)","LH (№4)","GND (№1)","LR (№2)","HR (№3)","SW (№1):","GND (№2):","1F (№3):","2F (№4):","1A (№1):","2A (№2):","+2.5 (№3):","GND (№4):","ALC (№5):","SMA (импульсный модулятор с BY)"]
[null,"0 - 6 ГГц","+3.3V (10mA)","+3.3V (10mA)",0,0,0,"?","?",0,0,"0..-0.9V","-1V..-0.2V","0..-0.9V","-1V..-0.2V","+2.5V",0,"-2.5V..0",1]
[null,"6 - 27 ГГц","+3.3V (10mA)","+3.3V (10mA)",0,1,0,1,0,1,0,"0..-0.9V","-1V..-0.2V","0..-0.9V","-1V..-0.2V","+2.5V",0,"-2.5V..0",1]
[null,"27 - 37 ГГц","+3.3V (10mA)","-3.3V (-10mA)",0,1,0,0,1,1,0,"0..-0.9V","-1V..-0.2V","0..-0.9V","-1V..-0.2V","'+2.5V",0,"-2.5V..0",1]
[null,"37 - 45 ГГц","-3.3V (-10mA)","+3.3V (10mA)",0,1,0,0,1,1,0,"0..-0.9V","-1V..-0.2V","0..-0.9V","-1V..-0.2V","+2.5V",0,"'-2.5V..0",1]
[]
[]
[{"$nulls":11},"1F -"]