{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":34,"n_cols":34,"rows_kept":34,"cut":false,"hidden":false,"merged":[[6,8,6,9],[7,8,7,9],[1,6,2,7],[1,8,2,9],[3,6,3,7],[4,6,4,7],[5,6,5,7],[3,8,3,9],[4,8,4,9],[5,8,5,9],[6,6,6,7],[14,2,15,33],[9,2,9,5],[9,10,9,19],[9,20,9,25],[10,2,10,5],[10,10,10,19],[10,20,10,25],[9,6,9,7],[9,8,9,9],[10,6,10,7],[10,8,10,9],[7,2,7,5],[7,10,7,19],[7,20,7,25],[8,2,8,5],[8,10,8,19],[8,20,8,25],[7,6,7,7],[8,6,8,7],[8,8,8,9],[19,2,29,13],[1,2,2,5],[3,2,3,5],[1,10,2,19],[1,20,2,25],[3,10,3,19],[3,20,3,25],[4,20,4,25],[4,2,4,5],[4,10,4,19],[5,2,5,5],[5,10,5,19],[5,20,5,25],[6,2,6,5],[6,10,6,19],[6,20,6,25]]}
[]
[null,null,"Имя объекта (Device ID)",null,null,null,"Адрес PCIE",null,"Адрес на ALINX",null,"Параметры передачи",{"$nulls":9},"Примечание"]
[]
[null,null,"SB_TMSG",null,null,null,"0x04",null,"0x01",null,"Длина слова 32 или 24 бита в завиcимости от cfgReg[1]"]
[null,null,"CfgReg",null,null,null,"0x08",null,"0x02",null,"Длина слова 32 бита",{"$nulls":9},"Конфигурационный регистр на ALINX"]
[null,null,"LMK_A",null,null,null,"0x10",null,"0x04",null,"Длина слова 24 бита",{"$nulls":9},"BOCHv2"]
[null,null,"LMK_B",null,null,null,"0x14",null,"0x05",null,"Длина слова 24 бита",{"$nulls":9},"BOCHv2"]
[null,null,"AttPe1",null,null,null,"0x1C",null,"0x07",null,"Длина слова 8 бит",{"$nulls":9},"Аттенюатор PE43711 (D13) на RFAMv1"]
[null,null,"AttPe2",null,null,null,"0x20",null,"0x08",null,"Длина слова 8 бит",{"$nulls":9},"Аттенюатор PE43711 (D17) на RFAMv1"]
[]
[]
[]
[]
[]
[null,null,"CfgReg"]
[]
[null,null,31,30,29,28,27,26,25,24,23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0]
[{"$nulls":27},"TmsgClk","SpiMode","HrGpio","LrGpio","Mod","WidthSpiTmsg","RstForFpga"]
[]
[null,null,"RstForFpga: сброс активный - лог.1 \nWidthSpiTmsg: 0 - 24 бит отгружается на SB_TMSG по SPI  \n                            1 - 32 бит отгружается на SB_TMSG по SPI\nMod: Управление импульснаям модулятором на RFAMv1\nLrGpio\nHrGpio\nSpiMode : 0 - 1Mosi\n                   1 - 4Mosi\nTmsgClk : 0 - 10MHz\n                  1 - 50MHz\n"]
{"$rows_empty":13}
[{"$nulls":22},"coo"]